TempoLink® smart assistant
Firmware: 1.5.29

Update:
- Support of G-Series V 
- Demo mode for demonstrating the TempoLink® smart assistant without connecting a sensor 
- Support of additional parameters of the R-Series V
- Improved display of sensors with stroke length > 3 m 


temposonics.com/tempolink


Updating the TempoLink® firmware
• Download the zip file and save it on your computer.
• Unzip the file.
• Connect your TempoLink® smart assistant to your
  computer via USB cable or via Wi-Fi (Recommendation:
  Use the Wi-Fi connection). A firmware update is not
  possible when connecting via smartphone or tablet.
• Click the UPDATE button. The “Configure TempoLink”
  window opens.
• Click the CHOOSE FILE button. Use the dialog to navigate to
  the location where you saved the firmware update file.
• Select the “update.tar” file. The selected file is displayed.
• Click the SUBMIT button to execute the update.
• The update process of the firmware consists of two steps:
  1. Transferring the update file to the TempoLink® smart
     assistant. This step is visualized via the progress bar.
  2. Installing the firmware. The LEDs on the TempoLink®
     smart assistant lights up orange.
  The update process normally takes 3 to 4 minutes.
  If you have your TempoLink® smart assistant connected to
  your computer via USB connection, during the installation,
  a USB drive will appear and disappear at your computer.
• After successful installation, the orange LEDs go out. LED
  A and LED B light up depending on the connection. LED C
  lights up green.
• If you have connected your computer to the TempoLink®
  smart assistant via Wi-Fi, restore the Wi-Fi connection
  after the installation is complete. The Wi-Fi connection is
  interrupted during the update.
• Refresh your browser by clicking the key combination
  CTRL + F5 and use the TempoLink® smart assistant
  as usual