____________________________________________________________

09 March 2007
ABB DTM TZIDC-110/210 PROFIBUS PA,  Revision: 1.00.20
With ABB DTM Library 2.00.36 and DTM Library Patch >= “2.00.3x Patch 5”
ABB Automation Products

Copyright (C) 1999-2007 ABB Automation Products
All Rights Reserved
______________________________________________________________________


--------------------------------------------------------------------------
Contents
--------------------------------------------------------------------------
1.  Supported devices
2.  Requirements
     2.1  PC-Hardware, Operating system
     2.2  Frame application / Compatibility
     2.3  Software package contents
3.  Installation and configuration
     3.1  Installation
     3.2  Linking Device/SK2 and SK1 hints
     3.3  Uninstall instructions
4.  Update / upgrade instructions
5.  What is new?
6.  Known problems or limitations
7.  Getting help / further information
8.  Licensing the DTM


---------------------------------------------------------------------------
1.  Supported devices
---------------------------------------------------------------------------
    Electro pneumatic positioner TZIDC-110, from firmware 1.00.00 and above.
    Electro pneumatic positioner TZIDC-210, from firmware 1.00.00 and above.

----------------------------------------------------------------------
2.  Requirements
----------------------------------------------------------------------
2.1  PC-Hardware, Operating Systems

- Minimum requirement
  Intel Pentium III Processor 450 MHz or compatible.
  256 MB RAM memory.
  300 MB free hard disk space.
  Windows 2000 / XP
  Internet Explorer 5.0.
  Adobe Reader  latest version
  Member of the "Administrators" group

The ABB DTM TZIDC-110 PA is released for Windows 2000 and
Windows XP Professional as PC / Notebook installation.

2.2  Frame application / Compatibility

The FDT 1.2 compatibility was tested with the dtmINSPECTOR 
Rev. 1.01.21.

Therefore the ABB DTM should be usable in all frame
applications according to the requirements of FDT 1.2.
Please read the respective frame application documentation, too.


----------------------------------------------------------------------
3.  Installation and configuration
----------------------------------------------------------------------
3.1  Installation

- Make sure that the minimum hardware requirements are met.
- Start Windows (login with administrator rights!).
- Cancel all running programs.
- Insert CD-ROM or unpack the DTM zip file available as download from
  www.abb.com/Instrumentation.
- Start "Setup.exe" in the directory \DTM\DTM TZIDC-PA (TZIDC-110,TZIDC-210)
  of the CD-ROM or in the directory you have chosen for the software 
  downloaded from the Internet.
- Follow the instructions.
  
3.2  Linking Device/SK2 and SK1 hints

- In case you intend to use PROFIBUS PA devices in a system 
  application and you are using a DP/PA Linking Device allowing a 
  DP Baud Rate > 93.25 kBaud, you need to convert the GSD-files of 
  the PA-devices.
  The DP/PA Linking Device may be:  
  - ABB Linking Device LD 800P
  - P&F coupler SK-2

  Following the installation of the DTM on your System, please 
  localize the GSD-file of the respective device. 
  Normally it is stored under the following path: 
    C:\Program Files\SMART VISION\SVDDesc\COM_DPV1\...\...\*.GSD
  The names of GSD-file usually contain the PNO-ID of the supported
  device.

  Example: 
  The GSD-file for the 2600T(265xx) is stored in the directory: 
    C:\Program Files\SMART_VISION\SVDDesc\COM_DPV1\_0016\_1_04c2 
  Filename: ABB_04C2.GSD 

- Implementation of the new GSD-file:
  The converted GSD-file made available by ABB and to find as 
  *GSD*.zip file on the CD-ROM in the device box or on the 
  following Internet address 
    http://www.abb.com/instrumentation.
  Please rename the original GSD-file 
   -> e.g. from "ABB_xxxx.GSD" to "ABB_xxxx.BAK" 
  Following this, rename the new GSD-file (e.g. YP00xxxx.GSD) with 
  the same name than the original GSD-file (ABB_xxxx.GSD) AND set the
  filedate to the current date. To do this, open save and close the 
  GSD-file (ABB_xxxx.GSD).

  Restart setup:
  Please restart the DTM setup with ‘setup.exe’


3.3  Uninstall instructions

- In the operating system: "Start -> Settings -> Control Panel 
  -> Add/Remove Programs -> Install/Uninstall" -> Select the DTM and
  Uninstall. 
  In any case uninstall all DTMs before uninstalling
  the frame application DSV401 R3 (SMART VISION).

----------------------------------------------------------------------
4.  Update / upgrade instructions
----------------------------------------------------------------------
- Uninstallation is not required before update / upgrade. It can be 
  handled like a new installation, existing projects will be kept. 

- When using a DP/PA Linking Device allowing a DP Baud Rate 
  > 93.25 kBaud:
  When updating / upgrading the PROFIBUS PA-DTM it is necessary to 
  re-install the converted GSD-file for Linking Devices in the 
  PA-DTM!
  Workflow see chapter "Linking Device/SK2 and SK1 hints"

- Hints regarding new versions may be found under 
  http://www.abb.com/Fieldbus

----------------------------------------------------------------------
5.  What is new?
----------------------------------------------------------------------
- Compatible to FDT 1.2 frame applications.
    
----------------------------------------------------------------------
6.  Known problems or limitations
----------------------------------------------------------------------
- Valid for FDT frame applications only:
  – TAG cannot be set via a DTM.
    In DSV401 R3 (SMART VISION) this limit does not apply.
  – DTM cannot switch to Offline mode if working with Online 
    Application. Device has to be disconnected first and then the DTM
    can be switched to Offline mode only.
    In DSV401 R3 (SMART VISION) this limit does not apply.
  – It could happen that the list of available functions for a DTM in 
    the frame application does not get updated. If that happens, click 
    on "New project" in the frame and when prompted to save click on 
    "Cancel". The DTM menu with all functions in the frame will be 
    available again.
    In DSV401 R3 (SMART VISION) this limit does not apply.
----------------------------------------------------------------------
7.  Getting help / further information
----------------------------------------------------------------------
- Press 'F1' for online help. Help concerning the integration of
  the DTM in the FDT frame application 
  (e.g. DSV401 R3 (SMART VISION), ...)
  can be found in the respective documentation of the frame 
  application.

  Hints regarding commissioning

- After connecting the device for the first time, an upload should be
  performed.
- After an upload of the device data into the DTM it is recommended to
  save all data.
----------------------------------------------------------------------
8.  Licensing the DTM
----------------------------------------------------------------------
- The DTM is usable without any license in any frame application.
- After the installation the ABB DTM runs 90-days in demo mode
  (full functionality) and needs to be purchased within this period,
  when the storage of data on a PC / Notebook being requested.
- By purchasing the DSV401 R3 (SMART VISION) single PC license
  the ABB DTM is also operable without restriction and does not have
  to be ordered separately!
____________________________________________________________
    End of file