First off all unzip this ZIP file!




System Requirements minimum
	- 2-GHz-Processor or better with 32 Bit (x86) or 64 Bit (x64)
	- 1 GB RAM or better
	- 500 MB free hard disk space
	- 1024 x 768 screen resolution recommended
	- Microsoft Windows 7 Service Pack 1, Windows 8.1 & Windows 10 (32 Bit / 64 Bit variants supported)
	- Microsoft .NET Framework 4.6.1
	- Microsoft Visual C++ 2015 Redistributables - 14.0.23026
	- Microsoft Internet Explorer 6.0 or higher
	- Adobe Reader latest version

Installation
	- Full administrator rights
	- Start of the installation wizard under the following path:
	    <drive>:\..3KXT161300S0202_DTM_TTx300-N-NINVA_HART.zipDTMTTx300NNINVAHART.exe

Further hints
	Further hints described in the “Supplementary Information” documents.
	Latest information and software available on:
	  www.abb.com/fieldbus

Note	
	Once installed the DTM runs 90-days in demo mode
	(full functionality) and must be purchased within this period,
	if the data storage on a PC / Notebook is requested.

In case of queries
	Please check ABB contact for Service in your country on
	http://www.abb.com/measurement



Copyright by ABB Automation Products GmbH: Use permitted according to terms of license, refer to data medium / ZIP file.


The device specific Version Matrix document helps you to find out what kind of software
is available for this field device and which software version you have to use with
which kind of Hardware and Firmware Revision.
The individual device driver Version Matrix (recommended), Supplement Info & Software is available latest on www.abb.com/fieldbus:
-> latest information [Field device protocol dependent]
   -> latest info (download) [device type dependent]
        - Driver description
        - Software [driver type dependent]
