First off all unzip this *.zip file!


The device specific Version Matrix document helps you to find out what kind of software
is available for this field device and which software version you have to use with
which kind of Hardware and Firmware Revision.
The individual device driver Version Matrix (recommended), Supplement Info & Software is available latest on www.abb.com/fieldbus:
-> latest information [Field device protocol dependent]
   -> latest info (download) [device type dependent]
        - Driver description
        - Software [driver type dependent]




You must use for Linking Devices/Segment Coupler with transfer rate 45.45 up to 12 MBaud 
  (e.g. ABB-LD800P, P+F-SK2, …)
    ->GSD-files YP0nxxxx.gsx

You must use for Segment Coupler with fixed transfer rate 45.45 or 93.75 Baud
  (e.g. ABB-NDL100-N, P+F-SK1, …)
    ->GSD-files ABB_xxxx.gsx

Additional information
- use acrobat reader to view the following documentations:
	
	-D184B093U29.pdf(datalink description in german language)
	-D184B093U30.pdf(datalink description in english language)
	

Date:    07.04.2009