____________________________________________________________

03 December 2008

ABB Engineer IT DTM FSM4000-HART,  Version 01.01.16
ABB Automation Products

Copyright (C) 1999-2008 ABB Automation Products
All Rights Reserved
____________________________________________________________


----------------------------------------------------------------------
Contents
----------------------------------------------------------------------
1.  Supported devices
2.  Requirements
     2.1  PC / Notebook
     2.2  Frame application / Compatibility
     2.3  Software package contents
3.  Setup and configuration
     3.1  Installation
     3.2  Installed files
     3.3  Uninstall instructions
4.  Update / upgrade instructions
5.  What is new?
6.  Known problems or limitations
7.  Getting help / further information
8.  Licensing the DTM
----------------------------------------------------------------------
1.  Supported devices
----------------------------------------------------------------------
- FSM4000 with HART communication
- with transmitter software revision B.1x - B.3x and C.1x
----------------------------------------------------------------------
2.  Requirements
----------------------------------------------------------------------
2.2.1  PC-Hardware, Operating Systems

- Minimum requirement
  Intel Pentium III Processor 450 MHz or compatible.
  256 MB RAM memory.
  300 MB free hard disk space.
  Windows 2000 / XP.  
  Internet Explorer 5.0. 
  Adobe Reader  latest version
  full administrator rights

The ABB FDT 1.2 DTM FSM4000-HART is released for Windows 2000 and 
Windows XP (Home / Professional) as PC / Notebook installation.

2.2  Frame application / Compatibility

The ABB FDT 1.2 DTM FSM4000-HART is released for DSV401 (SMART VISION) Release 3.

The FDT compatibility was tested with the dtmINSPECTOR Rev. 1.01.21. 
Therefore the ABB DTM should be usable in all Frame Applications according the requirements of FDT 1.2.
Please read also the respective Frame Application documentation.


2.3  Software Package Contents

The setup files are in the respective DTM sub directory.

- setup.exe

----------------------------------------------------------------------
3.  Setup and configuration
----------------------------------------------------------------------
3.1  Installation

- Make sure that the minimum hardware requirements are met.
- Start Windows (with administrator rights!).
- Close all running tasks.
- Insert CD-ROM. 
- Start "Setup.exe" in the DTM\DTM FSM4000-HART 
  directory of the CD or in the folder you choose for the software 
  downloaded from the Internet. 
- Follow the instructions.
  
3.2  Installed files

3.3  Uninstall instructions

- For uninstalling in the operating system: "Start-> Settings ->
  Control Panel -> Add/Remove Programs -> Install/Uninstall" ->
  Select the DTM and Uninstall. 
  In any case first uninstall all DTMs before uninstalling
  the frame application SMART VISION.

----------------------------------------------------------------------
4.  Update / upgrade instructions
----------------------------------------------------------------------
- Uninstallation is not needed before update / upgrade. It can be handled 
  like a new installation, existing projects will be kept. 

Hints regarding new versions may be found under 
http://www.abb.com/Fieldbus

----------------------------------------------------------------------
5.  What is new?
----------------------------------------------------------------------
- Compatible to FDT 1.2 frame applications.

Changes / Additionals / fixed bugs

11.04.03 (Version 01.00.00)
- initial release
23.04.03 (Version 01.00.01)
- download completed, bug fixed for adjust functions
26.05.03 (Version 01.00.02)
- new printfiles, new version of specification (Version 4.10)
17.09.03 (Version 01.01.00)
- device descriptions adapted
- automatic upload from device adjustable
- save to database always possible
- download-sequence adapted
- save data changes on exit adjustable
- address and order number readonly
- display the write protection (readonly)
- offline-parameter setting not available
- trend displays adapted
- display range adapted
18.09.03 (Version 01.01.01)
- date adjustable
14.10.03 (Version 01.01.02)
- visibility of pipe empty changed
- diagnosis frame changed
- warning at old software version implemented
- display programmable unit
- display values of detector pipe empty adjustment
- new value of Primary typ
- new value of Current output status at empty pipe 
09.02.04 (Version 01.01.03)
- with bundle license
- silent setup implemented (08/2005)
01.12.05 (Vers. 01.01.05)
- svd adapted (Html Print view function call as commented in svd file)
12/2007 (Vers 01.01.13)
- The DTM in Version 01.01.13 provides enhanced diagnosis functionality in correlation with hardware/firmware version C.10 .
These Functions are not available for Devices with lower Firmware Versions .
01/2009 (Ver. 01.01.16)
- several Bugfixes concerning the CSV output.

----------------------------------------------------------------------
6.  Known problems or limitations
----------------------------------------------------------------------
- Entries in edit boxes have to be acknowledged by Enter or TAB
  to be valid.
- If starting of a DTM fails with a runtime error 6 which 
occurs together with a control SV4_digital.OCX, the 
PC needs to reboot.   

----------------------------------------------------------------------
7.  Getting help / further information
----------------------------------------------------------------------
- Press 'F1' for online help. Help concerning the implementation of 
  the DTM in the FDT Frame Application (e.g. SMART VISION, ...)
  can be found in the respective documentation.

  Hints regarding commissioning

- When a device has been connected for the first time, and an upload
  was done, it is recommended to save all data using the menu 
  file/save as dataset. (database suffix *.dat)

- Initialisation of the DTM for the FSM4000:
  For starting the DTM, the DTM for the FSM4000as HART device has to
  be used when creating the project tree. For initialisation the point 
  "More" has to be selected in the menu under "Device". Depending on 
  the operating speed of the PC this could take some seconds.

- Configuration of the FSM4000:
  The DTM is started by clicking the right mouse key or via the menu 
  point "Device", in each case with "Edit".
  Changed data are displayed in blue and underligned. Using the command 
  "Save data to device" these data will be sent to the device.   


----------------------------------------------------------------------
8.  Licensing the DTM
----------------------------------------------------------------------

- The DTM is usable unlimited without any license in every Frame Application.
____________________________________________________________
End of file