TempoGate® smart assistant
Firmware: 1.5.26

Update:
-Hotfix for campatibility with browsers like Edge or Chrome

temposonics.com/tempogate


Updating the TempoGate® firmware
• Download the zip file and save it on your computer.
• Unzip the file.
• Connect your TempoGate® smart assistant to your computer via LAN or Wi-Fi.
  A firmware update is not possible when connecting via smartphone or tablet.
• Click the UPDATE button. The "Configure TempoGate" window opens.
• Click the CHOOSE FILE button. Use the dialog to navigate to the location where you saved the firmware update file.
• Select the file "update.cjb". The selected file is displayed.
• Click the SUBMIT button to execute the update.
• The update process of the firmware consists of two steps:
1. Transferring the update file to the TempoGate® smart assistant.
   This step is visualized via the progress bar.
2. Installing the firmware.
• After updating the firmware, this is indicated on the user interface by the message "Update Complete!".
• If you have connected your computer to the TempoGate® smart assistant via Wi-Fi,
  restore the Wi-Fi connection after the installation is complete.
  The Wi-Fi connection is interrupted during the update.
• Refresh your browser by clicking the key combination CTRL+F5 and use the TempoGate® smart assistant as usual.