First off all unzip this ZIP file!


Download ABB Filed Information Manager Version 3.2 following the below link:
https://search.abb.com/library/Download.aspx?DocumentID=7PAA018924&LanguageCode=en&DocumentPartId=&Action=Launch

After the download is success install Field Information Manager 3.2 by running 'ABB Field Information Manager Installer 3.2 (3.2.17292.0).exe'
Post installation import or drag and drop the FDI package [ABB.FMT700.01.01.00.GENERIC.fdix] available in this folder to FIM.

Refer document 7PAA000045D3200_A_en_Field Information Manager 3.2 - User Guide.pdf available in the installation setup folder of FIM under the folder Documentation.


Follow the instructions available in Appendix B [SetupofConnectivities], Section B.4 [ABBFIMBridgeSensyflowFMT700-P/FMT200-ECO2]/
B.4.1 SetupInstructions for setting up the communication.



Copyright by ABB Automation Products GmbH: Use permitted according to terms of license, refer to data medium / ZIP file.


The device specific Version Matrix document helps you to find out what kind of software
is available for this field device and which software version you have to use with
which kind of Hardware and Firmware Revision.
The individual device driver Version Matrix (recommended), Supplement Info & Software is available latest on www.abb.com/hart:
-> latest information [HART device protocol dependent]
   -> latest info (download) [device type dependent]
        - Driver description
        - Software [driver type dependent]


In case of queries
	Please check ABB contact for Service in your country on
	http://www.abb.com/measurement